|  |  |
| --- | --- |
| Parent Procedure(s):  | * CMS/314 OHS Injury Management Policy
 |

**1. INTRODUCTION**

*The OH&S Act 2004* requires that risks associated with hazards are to be eliminated or reduced where ‘reasonably practicable.

Sewer manholes vary in depth from approx 1 metre to 15 metres depending on the design of the reticulation system and topography and are generally of reinforced concrete construction. Access is generally by means of a small opening approx ¾ - 1 metre and step irons provide access to bottom of the well. Sewer mains generally run through the bottom of the well in the form of a channel. There may also be “internal drops” where a sewer inlet is cut into the wall of the well allowing flow of sewage downstream.

GWMWater Service Delivery employees routinely work around sewer manholes in carrying out a range of inspection and maintenance duties including sewer-jetting cleaning from the surface above the manhole.

In the development and implementation of this procedure, GWMWater aim to comply with the requirements of the OHS Regulations 2017 Part 3.3 *Prevention of Falls.*

**2. PURPOSE**

The purpose of this document is to:

1. Outline the fall prevention safety strategy to be undertaken by all GWMWater employees when working near a manhole
2. Provide guidance on process to protect workers from Biological waste exposure hazards

**3. SCOPE**

This work instruction applies to all GWMWater Manholes

   Typical Manhole



Sewer manhole barricade and manhole cover attached to sewer jetting trailer

Sewer manhole prevention of falls - Manhole cover and barricade

1. **SEWER MANHOLE PREVENTION OF FALLS AND CLEANING WORK INSTRUCTION**

**Setting Up**

* 1. Erect Telstra type barricade at manhole
	2. Workers wear suitable PPE (Disposable gloves & Eye protection)
	3. Gum boots required to be worn if attending sewer spills
	4. Remove manhole lid with appropriate lid tool
	5. Place manhole cover in manhole
	6. Ensure manhole cover is fitted appropriately to ensure a person cannot fall into manhole

**Pack Up**

1. Remove all equipment from manhole and pack up all equipment
2. Remove barricade from manhole area and store appropriately
3. Remove manhole cover
4. Immediately replace Permanent Manhole cover
5. Workers to clean tools, PPE and equipment used, by washing with low pressure water and wiped with disposable cloth to dry, before spraying with disinfectant and storing way.
6. Disposable cloths, gloves are placed into a suitably labelled container and covered with a lid.
7. Waste materials container is transported to appropriate disposal location and disposed of.
8. Workers are to wash hands thoroughly using soap and water before drying with paper towel or if no water and soap available, then use antibacterial hand soap on clean hands only
9. Report any damaged or poor fitting manhole covers to supervisor

**5. REFERERENCES**

* 1. *Occupational Health and Safety Act 2004 (Vic) s21 Duties of Employers to Employees*
	2. Occupational Health and Safety Regulations 2017 (Vic) Part 3.3 Prevention of Falls
	3. The National Code of Practice for the Prevention of Falls in General Construction
		1. (General Falls Code)